**Provided Materials**

Exterior

2”x4” Western Red Cedar floor joists

¾” Pressure-treated plywood subfloor

Nine prefabricated wall panels

Four exterior corner moldings

Three prefabricated roof panels

Metal roof package with peel-and-stick underlay

Roof fascia and soffit

Cedar deck boards pre-stained

Two cedar privacy walls pre-stained

Two cedar towel racks pre-stained

Prehung cedar door with glass insert pre-stained

Interior

Two prefabricated cedar floor panels with protective wax coating

Prefabricated upper and lower bench with protective wax coating

Prefacribated backrest with protective wax coating - black

Clear cedar finishing trim

Electrical

LED strip lighting preinstalled under the upper and lower benches

LED lighting driver

Bluetooth receiver and dimmable remote for LED strip lighting

PVC weatherproof box

Harvia Cilindor 9 KW electric sauna stove

4 boxes of 10-15mm sauna rocks

Hardware

We include every single piece of hardware you need to install ANGA!

**Required Tools**

Finishing Hammer

Tape Measure

Pencil

Utility Knife

Driver Drill

Two Step Ladders (one to access the roof 92” above ground)

Paint Brush

Hand Saw

Quick clamp (recommended but not required)

Chop Saw (recommended but not required)

18 Gauge Brad Nailer (recommended but not required)

Every piece of the sauna kit comes pre-assembled, pre-cut, and pre-drilled except for the interior finishing trim pieces. We highly recommend using a chop saw (mitre saw) to cut the trim pieces and an 18 gauge brad nailer to secure them. If you do not have access to either of these tools you can use a hand saw to cut the trim and a finishing hammer to install them.